Product program / Network Audio / IP Station

N-8610RM

IP remote microphone that employs packet audio technology.
High-quality voice output to intercom stations connected to the IP intercom exchange or Multi-Interface Unit and to other The unit shall be achieved by simply connecting the remote microphone to a LAN or WAN network. The IP Remote Microphone shall feature a full range of remote microphone operating capability, and be equipped with 14 function keys, including one under a cover, each with its own indicator. Functions shall be assigned individually to these keys. The number of function keys and indicators shall be increased to up to 40 in blocks of 10 with the addition of up to 4 RM-210 Extension Units. Power shall be supplied to the microhone using a PoE-compatible switching hub, eliminating the need for the dedicated optional AC adapter. It shall be wall-mounted with the additional use of the optional Wall-Mounting Bracket.