Product program / Network Audio / IP Station

N-8640SB

<div>The IP door station board is designed for use with TOA's packet intercom system (IP network compatible intercom system) that employs the packet audio technology and can be connected to an existing local area network (LAN) or wide area network (WAN).</div><div>Network shall be made possible using RJ45 connection via a switching hub.</div><div>Connecting the station to a switching hub with PoE functionality shall eliminate the need for an AC adapter. Network interface shall be I/F 10BASE-T/100BASE-TX (Automatic-Negotiation) Auto MDI/MDI-X compatible Network Protocol TCP/IP, UDP, ARP, ICMP, HTTP, RTP, IGMP.</div><div>The IP door station board unit shall be capable of automatic duplex hands-free conversation between the IP door station and IP master station or master stations connected to the intercom exchange.</div><div>The IP door station board unit allows the user to mount the unit into a customized housing of their choice and shall come complete with a 3.5 cm (1.38") cone-type speaker and an omni-directional electret condenser microphone allowing automatic duplex hands-free operation. It shall have 1 control input and 5 control outputs, including 1 relay channel, allowing connections to sensors such as electronic lock and other external equipment.</div><div>The IP door station board shall operate in temperatures between -10 ℃ to +50 ℃ with a relative humidity of 90 % or less.</div><div>Power requirements shall be 12 V DC from an optional AC adapter or by using a complaint PoE switching hub.</div><div>The dimension shall be 79 (W) × 134 (H) × 53 (D) mm (3.11" × 5.28" × 2.09") weighing 350 g (0.77 lb).</div><div>
</div><div>Optional extras: AD-1210P, AD-1215P AC adapter manufactured by TOA Corporation.</div>