Product program / Network Audio / IP Station

N-SP80MS1   QCU

SIP Multimedia Station with 7” Tochscreen
The SIP Multimedia Station shall be SIP compatible and Peer-to-Peer function shall be available.  It shall be equipped with capacitive 7” Tochscreen, Handset, 2M pixel free rotatable camera. The SIP Multimedia Station shall be PoE compatible and offer an optional DC Power supply. The internal address-book shall be capable of 3000 names storage. The IP Master Station must offer following Interfaces: Ethernet, WLAN, Bluetooth, HDMI, 3.5mm headset jack. Audio quality up to 7 kHz must be supported and an automatic echo canceller shall be available for noise free, intelligible conversation. 

Phone Features: Web support multi-language; Auto-answer; Volume control; Direct IP call without SIP proxy; Auto-Provision; DTMF modes: Inband, RFC2833, SIP INFO; Audio Features: VAD, CNG, AEC, G.165/G.168
Network Features: 2x10/100Mbps Ethernet Port; 1xPoE(IEEE803.2af); Security: Password Protection, IP address filtering; SIP over TLS; HTTPS encryption, user access log; Protocols support: IPv4, HTTP, HTTPS, FTP, DNS, NTP, RTSP, RTP, TCP, UDP, ICMP, DHCP, ARP; IP assignment: Static IP, DHCP, PPPoE
SIP Features: SIP v1(RFC2543), SIP v2(RFC3261); Audio codecs: G.711a, G.711μ, G.722, G.723, G.729a/b, iLBC, AMR-NB/WB, OPUS; Video codecs: H.263, H.264; Speech Quality: 7kHz Audio; Echo Cancellation; Voice Activation Detection; Comfort Noise Generator
Others: Android 4.2; Management by LCD Menu Configuration, WebUI; Download content from the specified server; Information receiving, storing, and rendering capabilities; Web browser; Contacts and Call records management; Support playing local or online video
Graphic Display: 7 inch capacitive touch screen TFT LCD, 800x480 pixels, 16:9 wide screen aspect ratio
Camera: 2M pixels C-MOS camera, free rotation
Resolution: up to 1080p
Video Features: QCIF, QVGA, CIF, 4CIF, VGA; Video bitrate: 64kbps~2Mbps; PIP; Full Screen; Local video ON/OFF control
Hands-Free: Microphone and Speaker built-in
Hand-set: Connected with a carl-cord
External Interface: IEEE802.11 b/g/n, USB 2.0, 3.5mm headset jack, HDMI
Power Source	: DC 12V by AC adaptor, PoE
Power Consumption: less than 12W
Installation: Desktop
Operating Temperature: 0℃ 40℃
Finish: ABS
Dimension: 240(H)x213(W)x120(D)mm
Manufacturer: TOA
Model: N-SP80MS1