Product program / Network Audio / IP Station

N-SP80VS1   Q

SIP Audio/Video Door Station for Building Access Control Communication and door remote control.
The IP Audio/Video Door Station shall be SIP compatible and Peer-to-Peer function shall be available. The Video-Camera shall be ONVIF compatible.
It shall be PoE compatible and offer an optional DC Power supply. The camera shall be a 3M pixel camera and automatic daylight check via photo sensor must be supported. Infrared light shall be activated automatically during darkness and support the video function. 
The IP Audio / Video Door Station shall be protected against water and dust according to IP65 grade. The call-button shall be free programmable. A multicolor status lamp shall be available and the status vs color shall be assignable.
The station shall offer 2x Control Inputs for alarm function and 2x Relays-Outputs for door opener function.
Audio quality up to 7 kHz must be supported and an automatic echo canceller shall be available for noise free, intelligible conversation. 

Phone Features: Web support multi-language; Auto-answer; Volume control; Direct IP call without SIP proxy; Auto-Provision
Network Features: 2x10/100Mbps Ethernet Port; Security: Password Protection, IP address filtering, SIP over TLS,HTTPS encryption, user access log; Protocols support: IPv4, HTTP, HTTPS, FTP, SNMP, DNS, NTP, RTSP, RTP, TCP, UDP, ICMP, DHCP, ARP
SIP Features: SIP v1(RFC2543), SIP v2(RFC3261); Audio codecs: G.711a, G.711μ, G.722, G.729; Video codecs: H.264 MPEG-4/MJEG (E21V only); Speech Quality: 7kHz Audio; Echo Cancellation; Voice Activation Detection; Comfort Noise Generator
Switches: 1 Call button, 1 reset button (on board)
Camera: 3M pixels
Resolution: up to 1080p
Microphone: 1 integrated microphone, IP67
Speaker: 1W, IP66
Control Input: 2 Control inputs for alarm
Control Output: 2 Relays outputs for door opener
Indication: Status lamp (colors: red, green, blue)
Power Source: 12V DC
Power Consumption: less than 12W
IP Grade: IP65
Installation: Flush-mounted, Fit in Clipsal 164/4 back box
Operating: -20℃ 55℃
Finish Plate: Stainless steel
Dimension: 210(H)x120(W)x45.6(D)mm