Product program / Digitales Audio-Konferenzsystem / NF-2S

NF-2S       1CE

Window Intercom System

The window intercom system shall consist of two sub-units, providing a loudspeaker and a microphone, and one base control unit.

The sub-units shall be attachable to partitions back-to-back without the use of tools by integrated magnets and thereby be reattachable. For the mounting on thick glass windows, additional self-adhesive magnets shall be included as accessory.

The base unit shall provide separate volume controls and mute buttons for both sub-units. One sub-unit shall be exchangeable with a custom headset. The base unit also shall provide a contact input for remote mute activation.

The window intercom system shall feature simultaneous two-way conversations with noise cancellation and echo cancellation. Internal equalizers shall counteract the loss of higher frequencies of the voice due to wearing a mask during conversations.

The system shall be extendable to a maximum of six connected sub-units in total.

An AC adapter and two 3.5 mm mini jack (4P) cables for the connection between base unit and sub-units shall be included.

Power source: 100 - 240 V AC, 50 / 60 Hz (use of supplied AC adapter)

Rated output: 1.7 W

Mic input: -30 dB, 3.5 mm mini jack (4P), phantom power supply

Speaker output: 16 Ω, 3.5 mm mini jack (4P)

Control input: External no-voltage mute input

Finish: [Base unit] ABS resin, white (case) and black (panel), paint / [sub-unit] ABS resin, white, paint

Dimensions (WxHxD): [Base unit] 127 mm x 30 mm x 137 mm / [sub-unit] 60 mm x 60 mm x 22.5 mm

Weight: [Base unit] 225 g / [sub-unit] 65 g

Manufacturer: TOA

Product: NF-2S