Product program / Amplifier / Power Amplifier

P-1812    ER

<div>The PA Amplifier shall deliver 120 W power output and be used in conjunction with the TOA A-1800 series PA Amplifiers.</div><div>It shall be mountable in a standard 19" equipment rack (2-unit size) using an optional rack mounting bracket.</div><div>Input level selector switch (–10 dB/0 dB) shall be provided to interface properly with different equipment.</div><div>On the back panel of the amplifier shall be a remote-in terminal for emergency control which sets the default output level for the emergency input.</div>