Product program / Amplifier / Power Amplifier

P-1812    ER

The PA Amplifier shall deliver 120 W power output and be used in conjunction with the TOA A-1800 series PA Amplifiers.It shall be mountable in a standard 19 equipment rack (2-unit size) using an optional rack mounting bracket.Input level selector switch (–10 dB/0 dB) shall be provided to interface properly with different equipment.On the back panel of the amplifier shall be a remote-in terminal for emergency control which sets the default output level for the emergency input.