Product program / Amplifier / Power Amplifier

P-2240    CE

<div>The booster amplifier shall operate on AC mains or 24 V DC power, and shall control and mix 1 balanced (screw terminal) Line in and 1 unbalanced (screw terminal) 100 V Line inputs. Outputs shall be balanced Loop out and balanced high and low impedance (floating) Speaker out. The amplifier shall meet the following performance criteria: Power output shall be 240 W at less than 1% THD (at 1 kHz, 1/3 rated power). Frequency response shall be 50 Hz to 20 kHz (+/-3 dB), with an S/N ratio of over 60 dB. Bass Tone Control shall be +/-10 dB at 100 Hz, and Treble Tone Control shall be +/-10 dB at 10 kHz. Power, signal and peak indicators, and fan cooling ventilation shall be provided. The panel shall be ABS black resin, and the case black steel plate. Dimensions shall be 420 (W) x 100.9 (H) x 351.3 (D) mm, and weight 13.2kg.&nbsp;</div><div>The booster amplifier shall be TOA model P-2240.</div>