Product program / Loudspeaker / Ceiling

PC-1869EN

Ceiling speakers for the voice alarm in 100 V technique, round, white metal front Grill with white metal ring (RAL 9010), quick and easy installation by spring clamping system, fire-resistant cable clamps made of ceramic, thermal fuse with a browing temperature of 72&deg;C.

The speaker must be certified by a notified body according to EN 54-24 and ISO 7240-24.
<p class="MsoNormal">

</p><p class="MsoNormal"/>