Product program / Loudspeaker / Ceiling

PC-2360

The loudspeaker shall be of in-ceiling type design, with a full lightweight metal construction with no visible fixings and a discreet outer bezel of only 5 mm.
Installation shall be via pre-mounted springs allowing it to be mounted in a ceiling with a thickness of between 5 – 25 mm (0.2" – 0.98"). A template shall be provided to assist in cutting mounting holes.
The loudspeaker shall incorporate a single 16 cm (6”) full range cone-type transducer with a smooth frequency response of 60 Hz to 20 kHz measured on axis.
The loudspeaker shall produce a Sound Pressure Level (SPL) of 94 dB on axis at 1 meter with a power input of 1 watt and shall be capable of producing 6 watts (for 100 V Line) and 3 watts (for 70 V Line) of power.
The loudspeaker shall be fitted with a factory mounted transformer with easy selectable power tappings of 6 W, 3 W, 1.5 W and 0.8 W when using 100 V Line and 3 W, 1.5 W, 0.8 W and 0.4 W when using 70 V Line. Push-in-type connectors shall make cable connection quick and easy and shall allow bridge connection when necessary.
The dimensions shall be φ230 × 76 (d) mm (9.06" x 2.99") weighing 740 g (1.63 lb.)
The finish of the loudspeaker shall be: Baffle: steel plate, white (RAL 9016 equivalent). Grille: Steel net, white (RAL 9016 equivalent).