Product program / Loudspeaker / Ceiling

PC-2369EN

Ceiling speakers for the voice alarm systems in 100 V technique, round, white metal front Grill with white metal ring (RAL 9010), easy installation with spring clamp system, fire-resistant cable clamps made of ceramic, high sound pressure and fidelity by 165 mm double cone diaphragm, thermal fuse with a blowing temperature of 72 °C.
&nbsp;
The speaker must be certified by a notified body (notified) according to EN 54-24 and ISO 7240-24.