Product program / Loudspeaker / Ceiling

PC-245AB-EB

<div>A/B line ceiling loudspeakers with fire pot and two loudspeakers and two 100V transformers for complete separation of the A and B loudspeaker lines. Cost-saving installation of a speaker by an A/B wiring instead of installing two speakers. Housing and fire pot made of steel. Cable connection via ceramic terminals with integrated thermal fuse.</div><div>
</div><div>The loudspeaker must be certified by a notified body in accordance with EN 54-24. The loudspeaker must meet the requirements of BS 5839-8:2013.
<p class="MsoNormal">Rated power: 2x 6 W

Tappings: 6 W, 3 W, 1.5 W

Nominal sound pressure: 88 dB (1W, 1m)

Frequency range: 150 - 20000 Hz

housing design: sheet steel, white painted &amp; nbsp; (similar to RAL 9016)

Dimensions (Ø x D): 245 x 131 mm

Installation opening: 220mm
</p><p class="MsoNormal">Certificate number: 1488-CPD-0335 / W

Notified body identified number: 1488
</p></div>