Product program / Loudspeaker / Ceiling

PC-275AB-EB

<div>A/B ceiling mounted loudspeaker with two separate loudspeakers and two separate 100V transformers to completely separate the A and B loudspeaker lines. Cost-saving installation of a speaker by an A/B wiring instead of installing two speakers. Steel housing. Cable connection via two ceramic terminals with integrated thermal fuse.</div>
<div>
</div>
<div>The loudspeaker must be certified by a notified body in accordance with EN 54-24. The loudspeaker must meet the requirements of BS 5839-8: 2013.

<p class="MsoNormal">Rated power: 2x 6 W

Tappings: 6 W, 3 W, 1.5 W

SPL: 88 dB (1W, 1m)

Frequency range: 180 - 20000 Hz

housing design: sheet steel, white painted &amp; nbsp; (similar to RAL 9016)

Dimensions (Ø x D): 280 x 86.5 mm
</p>
<p class="MsoNormal">Certificate number: 1488-CPD-0337 / W

Notified body identifier number Place: 1488
</p>
<p class="MsoNormal">Brand: TOA

Type: PC-275AB-EB</p>
<p class="MsoNormal"/>
<p class="MsoNormal"/>
</div>