Product program / Loudspeaker / Pendant

PE-154BS

The speaker shall combine a bass-reflex 12 cm (5") cone type, plus balanced dome tweeter, suitable for ceiling suspension mounting. It is also designed for use in voice evacuation systems. Input impedance shall be easily adjustable with rotary switch on the upper side of the speaker.
The speaker shall include a transformer having multiple taps (5 W, 10 W, 15 W at 100 V and 2.5 W, 5 W, 7.5 W at 70 V) adjustable. The output sound pressure level at a distance of 1 m with a 1 W input level applied shall be 91 dB SPL. The speaker shall have a frequency response of 70 – 20 kHz (-20 dB). The speaker shall have an ingress protection for indoor applications: IEC 60529 / EN60529 drip-proof rating of IP21C. 2 × fire-resistant steatite screw terminal blocks allows secure cable connections and bridge wiring. Thermal fuse with a blowing temperature of 84°C, 3 meters of shielded 4 core fire-resistant suspension cable avoid risk of failure of speaker line and provide secure mounting feature with internal flame-resistant insulated cables.
The speaker enclosure shall be constructed of HIPS resin. The grille shall be constructed of surface-treated steel plate net. The speaker shall be available in off-white colour. The unit shall have dimensions of ø186 × 251 (H) mm (ø7.32” × 9.88”), and a weight of 2.33 kg (5.14 lb).
The speaker shall be certified according to EN 54-24 with CPD Number 0359-CPD-0105, certified according to ISO 7240-24 and in compliance with the British Standard BS 5839-8: 2013.

The speaker shall be a TOA model PE-154BS