Product program / Loudspeaker / Pendant

PE-154EN

The speaker shall combine a bass-reflex 12 cm (5") cone type, plus balanced dome tweeter, suitable for ceiling suspension mounting. It is also designed for use in voice evacuation systems. Input impedance shall be easily adjustable with rotary switch on the upper side of the speaker.
The speaker shall include a transformer having multiple taps (5 W, 10 W, 15 W at 100V and 2.5 W, 5 W, 7.5 W at 70V) adjustable. The output sound pressure level at a distance of 1m with a 1 W input level applied shall be 91 dB SPL. The speaker shall have a frequency response of 70 – 20 kHz (-20dB). The speaker shall have an ingress protection for indoor applications: IEC 60529 / EN 60529 drip-proof rating of IP21C. A fire-resistant steatite screw terminal block allows secure cable connections and bridge wiring. Thermal fuse with a blowing temperature of 84°C. 5 meters sturdy suspension cable with internal flame-resistant insulated cables. The speaker enclosure shall be constructed of HIPS resin. The grille shall be constructed of surface-treated steel plate net. The speaker shall be available in off-white colour. The unit shall have dimensions of ø186 × 251 (H) mm (ø7.32” × 9.88”), and a weight of 2.1 kg (4.63 lb).
The speaker shall be certified according to EN 54-24 with CPD Number 0359-CPD-0105, certified according to ISO 7240-24.
The speaker shall be a TOA model PE-154EN.