Product program / Loudspeaker / Pendant

PE-304

The speaker shall be a bass-reflex 5" (12cm) cone type, plus balanced dome tweeter, suitable for ceiling suspension mounting. Input impedance shall be easily adjustable with rotary switch on the upper side of the speaker.
The speaker shall include a transformer having multiple taps (5W, 10W, 15W, 20W, 30W at 100V and 70V, and 8ohm) adjustable. The output sound pressure level at a distance of 1m with a 1W input level applied shall be 91 dB SPL. The speaker shall have a frequency response of 70 – 20,000Hz (-20dB). 
The speaker enclosure shall be constructed of HIPS resin. The grille shall be constructed of surface-treated steel plate net. The speaker shall be available in off-white color, and shall be easily repaintable. The unit shall have dimensions of ø186 x 251 (H) mm (ø7.32” x 9.88”), and a weight of 2.1 kg (4.63 lbs.).
The speaker shall be a TOA model PE-304.