Product program / Loudspeaker / Pendant

PE-64

The speaker shall be a bass-reflex 5" (12cm) cone type suitable for ceiling suspension mounting. Input impedance shall be easily adjustable with rotary switch on the upper side of the speaker. The speaker shall include a transformer having multiple taps (1W, 3W, 6W at 100V and 0.5W, 1.5W, 3W at 70V) adjustable. The output sound pressure level at a distance of 1m with a 1W input level applied shall be 90 dB SPL. The speaker shall have a frequency response of 100 – 18,000Hz (-20dB).
The speaker enclosure shall be constructed of HIPS resin. The grille shall be constructed of surface-treated steel plate net. The speaker shall be available in off-white color, and shall be easily repaintable. The unit shall have dimensions of ø186 x 251 (H) mm (ø 7.32” x 9.88”), and a weight of 1.5 kg (3.31 lbs.).
The speaker shall be a TOA model PE-64.