Product program / Loudspeaker / Projector

PJ-202DL-EB

Both-sided sound projector for outdoor and indoor use in robust aluminum housing with an IP44 protection degree. Wide temperature range from -25 ° C to + 70 ° C. Two coated 12 cm cone speakers with Mylar tweeter for weather resistance and high-quality sound transmission. Cable connection to ceramic terminal in watertight junction box. Integrated thermal fuse. The loudspeaker must be certified by a notified body in accordance with EN 54-24. The loudspeaker must meet the requirements of BS 5839-8: 2013. Rated load capacity: 20 W Power adaptation: 20 W, 10 W, 5 W Nominal sound pressure: 89 dB (1W, 1m) Transmission range: 120 - 20000 Hz housing design: cast aluminum, painted white <span>(similar to RAL 9016) Dimensions (Ø x D): 146 x 186 mm Certificate number: 1488-CPD-0338 / W Identification number Place: 1488 Brand: TOA Type: PJ-202DL-EB</span>