Product program / Loudspeaker / Horn

SC-630M   EB-Q

<p class="MsoNormal">Weatherproof horn speaker according to IP 65 for voice alarm, oval funnel made of powder-coated aluminum and driver cover made of ABS plastic, 70- and 100 volt operation possible, stainless steel swivel bracket for accurate Align the speaker, fire-resistant cable clamps made of ceramic, Thermal fuse with tripping temperature of 72 ° C, internal lines with Flame-retardant insulation in accordance with BS 5839 Part 8. A PG screw connection to the cable entry integrated, second PG cable gland to separate cable entry / exit optionally connectable.
</p>
<p class="MsoNormal">The speaker must go through, be a notified body certified to EN 54-24 and ISO 7240-24. The Speaker must meet the requirements of BS 5839-8.
</p>
<p class="MsoNormal">Rated Power: 15 W

Tappings: 15W, 10W, 5W, 3W

Degree of protection: IP 65

Frequency range: 315 - 12500 Hz

Sound pressure (1W, 1m): 109 dB

Type (EN 54-24): B (Outdoor)

Dimensions (W x H x D): 172 x 200 x 229 mm

PG cable gland <span>: Ø 6,5 - 12,5 mm &lt;/ span&gt;

Color: white
</span></p>
<p class="MsoNormal"><span>Certificate Number: 0359 - CPD- 0109

Notified body identification number : 0359
</span></p>
<p class="MsoNormal"><span>Brand: TOA

Type: SC-615BS</span></p>
<p class="MsoNormal"/>
<p class="MsoNormal"/>
<p class="MsoNormal"/>
<p class="MsoNormal"/>