Product program / Loudspeaker / Line Array

SR-C15B

The speaker shall be sub-woofer system. The component shall consist one 15" (38 cm) woofer. The speaker input connectors shall include screw terminal connections and two Neutrik NL4 type sockets. The speaker shall meet the following performance criteria. Power handling: 450 W continuous program. Frequency response (10 dB below rated pressure sensitivity, with recommended crossover and equalization) 40 to 400 Hz. Sensitivity (1 W at 1 m): 93 dB. Impedance: 8 ohms nominal.
The speaker enclosure shall be made of plywood and finished with black urethane paint. The speaker grille shall be made from a single punched steel plate and finished with black paint. The dimensions (W x H x D) shall be 526.6 x 594.8 x 550 mm (20.73" x 23.42" x 21.65") and weight (including accessory brackets) shall be 41 kg (90.39 lbs.). The speaker enclosure shall be equipped with M8 threaded steel plates for the secure attachment of optional accessory brackets. Available accessory brackets for suspension and stand mounting shall be made of steel.

The loudspeaker shall be TOA model SR-C15B.
The rigging frame shall be TOA model SR-RF8.