Product program / Loudspeaker / Line Array

SR-S4LEB-Q

Compact, straight line array loudspeaker element for true line array loudspeaker constructions (line sound source) in weatherproof design. Strong orientation of the radiation forward and sideways with low vertical radiation angle for sound in acoustically difficult environment. Small sound pressure decrease by distance (3 dB / distance doubling), thus more even sound pressure distribution than with conventional loudspeakers. Equipped with 8 x10-cm woofers and 24x tweeters. Internal crossover, but also controlled by two amplifiers with active crossover (bi-amp) possible. Connection via 4-core cable with a length of 3 meters. Optionally suitable 100-volt transformer can be installed. Various optional accessories for flying, wall and tripod mounting.

Frequency range: 70 - 20,000 Hz (-10 dB)
Rated power: 600 W
Impedance: 8 Ohm
SPL 1W, 1m: 94 dB 
Dispersion angle: 90 &deg; (hor.) X 0 &deg; (vert.)
Finish: MDF, painted white
Dimensions (W x H x D): 160 x 895 x 255 mm
Weight: 16 kg
Protection level IPx4
Type (EN 54-24): A

Brand: TOA
Type: SR-S4LWPEB-Q

Certificate number: 1488 / CPR / 0570 / W
Identifier notified body: 1488