Product program / Loudspeaker / Line Array

SR-S4LWP

Compact, straight line array speaker element in column form for true line array loudspeaker designs (sound source) in weatherproof execution. Strong alignment of radiation to the front and sides with low vertical angle for PA applications in acoustically difficult environments. Low sound pressure decrease with distance (3 dB / doubling of distance), so even sound pressure distribution than with conventional speakers. Equipped with 8-inch of Woofer and 24 tweeters. Internal crossover, but also control through two amplifiers with active crossover (bi-amp) easily. Connection via 4-core cable with a length of 3 meters. Optional matching 100-volt transformer can be mounted. Diverse optional accessories for flying as well as wall and tripod mount.
&nbsp;
Frequency range: 70-20,000 Hz (-10 dB)
Capacity: 600 W
Impedance: 8 ohm
Nominal SPL, 1W, 1 m: 94 dB SPL
Beam pattern: 90&deg; (hor.) x 0&deg; (vert.)
Finish: MDF, painted white
Dimensions (W x H x D): 160 x 895 x 255 mm
Weight: 16 kg
Degree of protection IPx4
&nbsp;
Manufacturer: TOA
Model: SR-S4LWP