Product program / Loudspeaker / Line Array

SR-S4SEB-Q

Compact, curved line array speaker element in columnar form for real line array loudspeaker constructions (line sound source) in weatherproof design. Strong orientation of the radiation forward and sideways with low vertical radiation angle for sound in acoustically difficult environment. Low sound pressure decrease with distance (3 dB / distance doubling), thus more even sound pressure distribution than with conventional loudspeakers. Equipped with 8 10-cm woofers and 24 tweeters. Internal crossover, but also controlled by two amplifiers with active crossover (bi-amp) easily possible. Connection via 4-core cable with a length of 3 meters. Optionally suitable 100-volt transformer can be installed. Various optional accessories for flying, wall and tripod mounting.
Frequency range: 70 - 20,000 Hz (-10 dB)
Rated power: 600 W
Impedance: 8 Ohm
SPL 1W, 1m: 93 dB
Dispersion angle: 90 &deg; (hor.) X 10 &deg; (vert.)
Finish: MDF, painted white
Dimensions (W x H x D): 160 x 892 x 255 mm
Weight: 16 kg
Protection level IPx4
Type (EN 54-24): A

Brand: TOA
Type: SR-S4SWPEB-Q

Certificate number: 1488 / CPR / 0570 / W
Identifier notified body: 1488