Product program / System Component / Control and Indication Units

SX-2000CI

Control input unit for installation in 19-inch cabinet racks (IEC 60297) with 32 control inputs with opto-couplers. Each input can be monitored either. The activation of each single control input will be shown at the front by means of LEDs. The connection is via detachable connectors.
Redundant power supply for reliable power supply. Supervised access to the system via RJ45 jacks. Additional RJ45 connector for control output unit.
Regulated voltage output to the supply of external devices. More ads for supply voltage, collective fault signal and activated analog reserve way.