Product program / System Component / Control and Indication Units

SX-2000CO

Control output unit for installation in 19-inch cabinet racks (IEC 60297) with 32 control outputs via relay changeover contacts, so that normally closed and normally open can be used. The activation of each single control output will be shown at the front by means of LEDs. The connection is via detachable connectors. Redundant power supply for reliable power supply. Supervised access to the system via RJ45 jacks. Additional RJ45 connector for control input unit. More ads for supply voltage, collective fault signal and activated analog reserve way.