Product program / System Component / I/O Modules

SX-200RM

Speaking points input module for the connection of two receivers. Connecting and powering the System receivers from two RJ45 Sockets. Gain control (gain) for each port, 24-bit AD-converter per channel.
&nbsp;
Input sensitivity: 0 dBV
ADC: 24 bit, 48 kHz
Gain adjustment (gain): 0... + 12 dB
Power stations: 1 A (max.) per connection
&nbsp;
Manufacturer: TOA
Model: SX-200RM