Product program / System Component / I/O Units

SX-2100AI

Fully digital audio input unit for installation in 19-inch cabinet racks (IEC 60297) for up to 8 audio sources.
Two network connections (100BaseTX) for redundant network for audio and control signals, additional analog reserve way. Redundant power supply for reliable power supply.
16 Control inputs and 16 control outputs with relay contact, normally closed or normally open freely selectable via detachable connectors.
Four slots for dual-channel modules for a goose, suitable for various signal sources from MIC to line level with various inputs removable screw terminal blocks, XLR and RCA jacks.
Large multicolored display on the front of the machine for:
-18-digit text display for system information
-Modulation bar indicator for each of the 8 channels
-Status of each channel (on/off)
-Status of network channels
-Collective fault signal
-Communication error (data line)
-Emergency mode
Buttons to select of the display of the system information. Separate display for power supply, standby (standby) and activated analog reserve way.
Four function keys to choose of pre-programmed music transfers or activation of transmissions from an entrance on pre-programmed areas. 8 Channel keys to the switching on and off individual channels, optionally umprogrammierbar on activation of transmissions from an entrance on pre-programmed areas. Volume control for each channel, which is bridged for emergency-related transfers. Access to all the controls can be locked. 
Built-in monitor speakers with volume control to listen to each channel.
Compliant monitoring of all alarm-relevant signaling pathways, CPU, power supply and network connections.