Product program / System Component / System Manager / Central Unit

TS-770    CE

The central unit shall be designed to be connected with the chairman unit, the delegate units and the remote delegate interface unit to form a complete conference system that allows normal in-house conference use, as well as conference participation by parties in remote locations via a telephone line or PC. The unit shall be small in size to enable easy installation and storage. Up to 3 central units shall be able to be connected simultaneously per system. The central unit shall operate on AC mains and shall be rated at an output of 35V DC. The power consumption shall be 60W (maximum). The central unit shall be equipped with 2 audio inputs, 3 recording outputs (phone jack/pin jack selectable), 1 equalizer input, 1 equalizer output, 2 expansion inputs, 2 expansion outputs and 2 control outputs. An internal chime shall be sounded when the chairman unit’s priority button is pressed to allow the chairman unit to take precedence over any delegate unit. The operating temperature range shall be between 0&deg;C and +40&deg;C and the operating humidity shall be under 90 percent. The panel shall be hairline patterned aluminum painted in black, while the case shall be precoated steel plate painted in black. The dimensions shall be 210 (W) x 107.1 (H) x 316 (D) mm and the weight shall be 4 kg.
The central unit shall be a TOA TS-770 or approved equivalent.