Product program / System Component / Interface

TS-775

The specified remote delegate interface unit shall enable parties in remote locations to participate in conferences via a telephone line or PC. The remote delegate interface unit shall operate on 35V DC supplied from the central unit and shall be fitted with 1 input and 1 output, plus their respective volume controls. The remote delegate interface unit shall also be fitted with a speech mode selector switch which automatically reverses voice-controlled speech flows when set to the auto position and allows speech to be manually initiated or terminated by pressing the talk key when set to the manual position. The operating temperature range shall be between 0&deg;C and +40&deg;C and the operating humidity shall be under 90 percent. The case shall be made of pre-coated steel plate painted in black and the weight shall be 700 g. The dimensions shall be 160 (W) x 41.8 (H) by 100 (D) mm.
The remote delegate interface unit shall be a TOA TS-775 or approved equivalent.