Product program / System Component / System Manager / Central Unit

TS-800    CE

Central control unit the infrared conference system

in sturdy metal enclosure to the desk top or 19-inch rack cabinet mounting with optional installation brackets with a space of 4 Unit. Designed for the operation of up to 64 participants-stations, as well as unlimited passive listeners. 
Controls, indicators and features:
Limit the simultaneous transmission of 1, 2, or 4 intercoms can be set. When exceeding the limit, one of the three priority settings can be selected:
-Blocking later enabled transfers
-Unlock of later enabled transfers through the completion of the first broadcasts
-Maintaining the first transfer and unlock of later enabled transfers by stopping the transfer following the first transmission
Automatic microphone can be activated either after speech. Central volume control for the speaking points speaker. Display of operating status of the four transmission channels, the transmission of control signals and battery condition of the stations. Switch with power indicator and headphone jack with volume control.
Function for checking the proper communication between the stations and the central unit.

Inputs and outputs: Central control unit the infrared conference system

in sturdy metal enclosure to the desk top or 19-inch rack cabinet mounting with optional installation brackets with a space of 4 Unit. Designed for the operation of up to 64 participants-stations, as well as unlimited passive listeners. 

Controls, indicators and features:
Limit the simultaneous transmission of 1, 2, or 4 intercoms can be set. When exceeding the limit, one of the three priority settings can be selected:
-Blocking later enabled transfers
-Unlock of later enabled transfers through the completion of the first broadcasts
-Maintaining the first transfer and unlock of later enabled transfers by stopping the transfer following the first transmission
Automatic microphone can be activated either after speech. Central volume control for the speaking points speaker. Display of operating status of the four transmission channels, the transmission of control signals and battery condition of the stations. Switch with power indicator and headphone jack with volume control.
Function for checking the proper communication between the stations and the central unit.

Inputs and outputs:
Separately controllable inputs to outputs for connecting recording devices (E.g. log recorder) and Lautsprecher-Anlagen, a microphone and a playback device (E.g. CD player). 4 BNC connectors for infrared transceivers, of which up to 16 IR transceiver via distribution can be connected.
Serial interface RS 232 for optional control of the Conference system by means of operating computer or media control.
Power supply unit included.