Product program / System Microphone / Conference

TS-801    CE

The Chairperson Unit shall be easily installed and removed. The Chairperson Unit shall feature a priority speech key, which allows it to take precedence over the Delegate Unit when speaking. The Chairperson Unit shall provide microphone-input terminal using the combined type of XLR-4-31 connector for the (optional) standard microphone or the (optional) long microphone. The Chairperson Unit shall include a monitor speaker: 8 ohm, 0.2 watt and (2) headphone Mini Jack. The Chairperson Unit shall include an LED indicator, which shall provide a speech indicator, power indicator / low battery indicator and out of communication range indicator. The Chairperson Unit shall be operated on either the AC adapter (optional) or the lithium-ion battery (optional). The Chairperson Unit shall be equipped with a remaining battery indicator. Two types of dedicated microphones shall be available as optional products: the standard type and the long type. Power requirement shall be 7.4VDC (optional) battery, 9VDC (optional) AC adapter. The Chairperson Unit shall weigh 1.39 lbs. (630g) and shall be finished: Top Panel: ABS resin, gray metallic, paint, semi-matte with dimensions (W x H x D) 8.3” x 2.6” x 6” (210 x 65.9 x 152 mm).