Product program / System Microphone / Conference

TS-802    CE

The Delegate Unit shall be easily installed and removed. The Delegate Unit shall provide: Microphone Input terminal using the combined type of XLR-4-31 connector for the (optional) standard microphone or the (optional) long microphone. Monitor speaker: 8 ohm, 0.2 watt and (2) headphone Mini Jack. The Delegate Unit shall include an LED indicator, which shall provide a speech indicator, power indicator / low battery indicator and out of communication range indicator. The Delegate Unit shall be operated on either the AC adapter (optional) or the lithium-ion battery (optional). Two types of dedicated microphones shall be available as optional products: the standard type and the long type. Power requirement shall be 7.4VDC (optional) battery, 9VDC (optional) AC adapter. The Delegate Unit shall weigh 1.39 lbs. (630g) and shall be finished: Top Panel: ABS resin, gray metallic, paint, semi-matte with dimensions (W x H x D) 8.3” x 2.6” x 6” (210 x 65.9 x 152 mm).