Product program / System Microphone / Conference

TS-811

The Chairperson Unit shall be connected to the dedicated Bridge Unit by a CAT5 cable.The Chairperson Unit shall feature a priority speech key, which allows it to take precedence over the Delegate Unit when speaking. The unit shall have base language/translation language selection function. The Chairperson Unit shall provide microphone-input terminal using the combined type of XLR-4-31 connector for the (optional) standard microphone or the (optional) long microphone. The Chairperson Unit shall include a monitor speaker: 8 ohm, 0.2 watt and 2 (two) headphone Mini Jacks. The monitor speaker volume and 2 headphones output volume shall be ajustable.&nbsp; The Chairperson Unit shall include an LED indicator, which shall provide a speech indicator, power indicator / low battery indicator and out of communication range indicator. Built-in DIP switch on its bottom shall enable the following settings: Priority operation setting, Priority chime mute setting, Voting activation setting, and Priority speech key operation setting. The Chairperson Unit shall operate on 24V DC, supplied from an Expansion Unit. Two types of dedicated microphones shall be available as optional products: the standard type and the long type. The Chairperson Unit shall weigh 640g (1.41 lbs.) and shall be finished: Top Panel: ABS resin, gray metallic, paint, semi-matte with dimensions (W x H x D) 210 x 65.9 x 152 mm (8.27" x 2.59" x 5.98").

The Chairperson Unit shall be the TOA model TS-811.
The Expansion Unit shall be the TOA model TS-918.
The Bridge Unit shall be the TOA model TS-919B1/919B4.