Product program / System Component / Accessory

TS-907

The Infrared Transmitter / Receiver Unit shall include the following functionality: Facilitates wireless communication between the Chairperson Unit and Delegate Unit. The Infrared Transmitter / Receiver Unit connects to the Central Unit using coaxial cable. Compatible coaxial cable types shall include: RG-59/U, RG-6/U and RG-11/U. The Infrared Transmitter / Receiver Unit can be mounted using the following configurations: Ceiling Mounted, Wall Mounted using the supplied mounting bracket or Mounted to an optional Microphone Stand using the supplied stand mounting bracket. The optional Microphone Stand mounting thread size shall be W 5/16. Power requirement shall be 24VDC, maximum 100 mA supplied from the Central Unit via the coaxial cable. The Infrared Transmitter / Receiver Unit shall weigh 0.5 lbs (230 g) and shall be constructed of: Dome shall be PC resin, visible light cut filter. Base: ABS resin, black with dimensions&nbsp; 4.72” diameter (120mm) x&nbsp; 2.8” height (71.3mm).

The Infrared Transmitter/Receiver shall be the TOA model TS-907.