Product program / System Microphone / Conference

TS-921      Y

The Chairperson Unit shall feature a priority speech key, which allows it to take precedence over the Delegate Unit when speaking. The unit shall have base language/translation language selection function. The Chairperson Unit shall provide microphone-input terminal using the combined type of XLR-4-31 connector for the (optional) standard microphone or the (optional) long microphone. The Chairperson Unit shall include a monitor speaker: 8 ohm, 0.2 watt and 2 headphone Mini Jacks. The monitor speaker volume and 2 headphones output volume shall be adjustable. The Chairperson Unit shall include an LED indicator, which shall provide a speech indicator, power indicator / low battery indicator and out of communication range indicator. Built-in DIP switch on its bottom shall enable the following settings: Priority operation setting, Priority chime mute setting, Voting activation setting, and Priority speech key operation setting. The Chairperson Unit shall operate on 7.2V DC (using the optional Lithium-Ion Battery) or 9V DC (using the optional AC Power Supply). Two types of dedicated microphones shall be available as optional products: the standard type and the long type. The Chairperson Unit shall weigh 550g (1.21 lbs.) and shall be finished: Case: PC resin, black, with dimensions (W x H x D) 205.7 x 70.3 x 164.2 mm (8.10" x 2.77" x 6.46").

The Chairperson Unit shall be the TOA model TS-921.
The standard microphone shall be the TOA model TS-923.
The long microphone shall be the TOA model TS-924.
The AC Power Supply shall be the TOA model AD-0910.
The Lithium-Ion Battery shall be the TOA model BP-900A.