Product program / System Microphone / Conference

TS-D1000-DU Y

The delegate unit shall provide microphone-input terminal using the combined type of XLR-3-31 connector for the (optional) standard microphone or the (optional) long microphone. The delegation unit shall support voice activation. The delegate unit shall include a monitor speaker: 8 ohm, 0.4 watt and 2 headphone mini Jacks. The monitor speaker volume and 2 headphones output volume shall be adjustable. Built-in DIP switch on its bottom shall enable the following settings: Priority operation setting, priority chime mute setting and priority speech key operation setting. The delegate unit shall operate on 24V DC (supplied from the master control unit, sub control unit or extension unit). Two types of dedicated microphones shall be available as optional products: the standard type and the long type. The delegate unit shall weigh 875g (1.93 lbs.) and shall be finished: Case: ABS resin, black, mat finish; speaker net: Black, matt finish with dimensions (W x H x D) 208.9 x 71.3 x 160.5 mm (8.22" x 2.81" x 6.32").

The delegation unit shall be the TOA model TS-D1000-DU. The standard microphone shall be the TOA model TS-D1000-M1. The long microphone shall be the TOA model TS-D1000-M2. The master unit shall be the TOA model TS-D1000-MU. The sub control unit shall be the TOA model TS-D1000-SU. The extension unit shall be the TOA model TS-D1000-EX.