Product program / System Component / Interface

TS-D1000-EX 4CE

The expansion unit shall extend a single line to up to 100m (328 ft). It shall be connected at the end of a daisy chain wiring line between the master/sub control unit and chairman/delegate units wit CAT5e STP LAN cables. It shall be powered with 100-240 V AC at 50/60 Hz with the supplied AC adapter and shall supply the chairman/delegate units with 24 V DC. The expansion unit shall be the TOA model TS-D1000-EX, the chairman/delegate units shall be the TOA models TS-D1000-CU/DU and the master unit shall be the TOA model TS-D1000-MU.