Product program / System Microphone / Conference

TS-D1000-M1

The gooseneck microphone shall come with red lights ring to display speech indicator, connection test indicator and one flexible section. The microphone chall use a XLR-3-32 connector for connection to the delegate and chairperson units. Sensitivity:-37 dB (1 kHz, 0 dB = 1 V / PA) Frequency response: 100 Hz - 13 kHz Finish: Gooseneck: black, stainless steel; Other: ABS resin, black. Length: 518 mm (20,39") Weight: 110 g (0.24 lb)

The standard microphone unit shall be the TOA model TS-D1000-M1.