Product program / System Microphone / Conference

TS-D1000-M2

The gooseneck microphone shall come with red lights ring to display speech indicator, connection test indicator and one flexible section. The microphone chall use a XLR-3-32 connector for connection to the delegate and chairperson units. Sensitivity:-37 dB (1 kHz, 0 dB = 1 V / PA) Frequency response: 100 Hz - 13 kHz Finish: Gooseneck: black, stainless steel; Other: ABS resin, black. Length: 668 mm (2,19ft) Weight: 125 g (0.28 lb).

The long microphone unit shall be the TOA model TS-D1000-M2.