Product program / System Component / Interface

TS-D1000-SU 1CE

The sub control unit shall connect up to 48 additional conference units to the master unit by using CAT5e STP LAN cables. The power source shall be 100-240 V AC at 50/60 Hz and the units power consumption shall be 80 W at maximum. With the use of an optional rack mounting bracket, it shall be mounted in an EIA standard equipment rack (1-unit size). The sub control unit shall be the TOA model TS-D1000-SU, the conference units shall be the TOA models TS-D1000-CU/DU and the master unit shall be the TOA model TS-D1000-MU.