Product program / System Microphone / Conference

TS-D1100-MC Y

<div>TS-D1100-MC&nbsp;</div><div>Microphone Unit&nbsp;

</div><div><div>The microphone unit shall feature a compact design for desktop placement and shall provide an integrated gooseneck microphone. The unit shall provide a talk key that activates the microphone after pressing and deactivates microphone after pressing the key again. There shall be two connection ports that allow connection to the main unit and daisy chain connection to another conference unit.&nbsp;

</div><div><div>Power source: Supplied from system&nbsp;</div><div><div>Power consumption: 0.4 W or less&nbsp;</div><div><div>Frequency response: 100 Hz, max. to 13 kHz, min.&nbsp;</div><div><div>LED Indicator: Power and speech indicator&nbsp;</div><div><div>Operating temperature: 0 &deg;C, max. to 40 &deg;C. min.&nbsp;</div><div><div>Finish: [shaft] brass, black / [case] ABS resin, black&nbsp;</div><div><div>Dimensions (WxHxD): 114 mm x 516 mm x 145.9 mm or less&nbsp;</div><div><div>Weight: 330 g or less&nbsp;</div><div><div>&nbsp;</div><div>Manufacturer: TOA&nbsp;</div><div>Product: TS-D1100-MC&nbsp;</div></div></div></div></div></div></div></div></div></div></div>