Product program / System Component / System Manager / Central Unit

TS-D1100-MU 4CE

Conference System Master Control Unit

The master control unit shall support the connection of at least 32 wired conference units and at least 246 conference units while using additional sub control units. Delegate units and multiple chairman units shall be connectable.

At least four different conference modes shall be available: First-in-first-out priority, last-in-first-out priority, voice activation and chairman only. At least 8 conference units shall be able to speaker simultaneously. The number shall be limitable to at least 1 or 2 manually via the master control unit.

The master control unit shall provide an integrated feedback suppression. Furthermore, it shall be possible to insert a DSP device into the signal chain to add additional signal processing.

The master control unit shall provide the recording of conferences on its internal storage or a locally installed USB drive (at least 32 GB capacity shall be supported).

The master control unit shall provide a USB interface to enable the integration of online conference participants via a computer. The configuration of the device using a computer shall be possible via TCP/IP connection.

Power source: At least 100 - 240 V AC, 50/60 Hz

Power consumption: 60 W or less

Frequency response: At least 100 Hz - 13 kHz

Audio inputs: At least 1x Mic (phone jack), 1x EQ input (RCA), 1x Video conference input (RCA)

Audio outputs: At least 1x Line (phone jack), 1x Rec (RCA), 1x Headphones (mini jack), 1x EQ output (RCA), 1x Video conference output (RCA)

Digital audio interface: USB 2.0, type-B port

Network I/F: 100BASE-TX, Auto MDI/MDI-X, RJ45 connector

Network Protocol: TCP, HTTP, DHCP, ARP (APIPA), UDP (mDNS), UPnP

Finish: (Panel) Steel plate, 30 % gloss, surface-treated, paint, black

Dimensions (WxHxD): 361 mm x 100.4 mm x 184.2 mm or less

Weight: 2.2 kg or less

Manufacturer: TOA

Product: TS-D1100-MU