Product program / System Microphone / Conference

TS-D1100-SP Y

<div>TS-D1100-SP&nbsp;</div><div>Speaker Unit&nbsp;

</div><div><div>The speaker unit shall feature a compact design for desktop placement and shall be able to cover a radius of 3 m or more regarding sound broadcasting. The unit shall provide volume control with six selectable levels or more. There shall be two connection ports that allow connection to the main unit and daisy chain connection to another conference unit.&nbsp;

</div><div><div>&nbsp;Power source: Supplied from system&nbsp;</div><div><div>Power consumption: 5 W or less&nbsp;</div><div><div>Speaker output: 1 W or more&nbsp;</div><div><div>Frequency response: 100 Hz, max. to 13 kHz, min.&nbsp;</div><div><div>LED Indicator: Power and volume&nbsp;</div><div><div>Function keys: 1x volume up, 1x volume down&nbsp;</div><div><div>Operating temperature: 0 &deg;C, max. to 40 &deg;C. min.&nbsp;</div><div><div>Finish: ABS resin, black&nbsp;</div><div><div>Dimensions (WxHxD): 214.2 mm × 55.3 mm × 211.4 mm or less&nbsp;</div><div><div>Weight: 550 g or less&nbsp;</div><div><div>&nbsp;</div><div>Manufacturer: TOA&nbsp;</div><div>Product: TS-D1100-SP&nbsp;</div></div></div></div></div></div></div></div></div></div></div></div></div>