Product program / Loudspeaker / Accessory

TU-631M

<div>The Driver Unit shall be designed to be used in combination with an optional round horn. The driver unit/horn combined speaker can be used for both indoor and outdoor applications, as well as for background music reproduction. The driver lineup shall include four models rated at 30 W and 50 W. The models designed for use in high-impedance (70V/100V lines) systems and standard models for low-impedance (16 Ω) systems shall be available. This wide product lineup shall permit selection of the ideal speaker for most applications.</div><div>
</div><div>The Driver Unit shall featur newly developed diaphragms employing special heat-resistant polyimide film to prevent the diaphragm from absorbing moisture and changing shape, as well as to improve the low frequency characteristics. High speaker efficiency shall have also been realized by minimizing the gap produced when the diaphragm bobbin is installed in the magnetic circuitry slit. High-impedance models shall be equipped with an input impedance selector switch which facilitates impedance settings without requiring disassembly. The switch shall be also equipped with an OFF position to prevent speaker damage resulting from incorrect impedance setting.</div><div>
</div><div>The Driver Unit shall be the TOA model TU-631/631M/651/651M.</div>