Product program / Loudspeaker / Column

TZ-400BS-EB

Column speaker, 20 W, EN54
The speaker shall be a wall mount column speakers designed for indoor and outdoor installation. The speakers shall come with screw type loop through steatite terminal block and thermal fuse. They shall be certified according to the European Standard EN 54-24:2008 and compliant with the British Standard BS 5839-8:2008. 

Rated Input:  Min. 40 W 

Rated Impedance: 100 V line: Min. 250 Ω (40 W), 500 Ω (20 W), 1 kΩ (10 W)
&nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp;70 V line: Min. 250 Ω (40 W), 500 Ω (10 W), 1 kΩ (5 W)

Frequency Response:	  Max. 110 Hz – min. 20 kHz (Peak – 20 dB) 

Sensitivity: Min. 93 dB (1 W, 1m, 100 – 10 kHz, pink noise) 
			
Max. SPL: Min. 109 dB (20 W, 1m, 100 – 10 kHz, pink noise) 
		
Coverage Angle (-6 dB):  
&nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp;500Hz:Horizontal 360&deg;, min. Vertical 100&deg; 
&nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp;1kHz: Min. Horizontal 185&deg;, min. Vertical 45&deg; 
&nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp;2kHz: Min. Horizontal 130&deg;, min. Vertical 25&deg; 
&nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp; &nbsp;4kHz: Min. Horizontal 100&deg;, min. Vertical 20&deg;

Operating Temperature: Max. -30 &deg;C – min. 60 &deg;C

Dust/Water Protection: Min. IP 66

Environmental Type: Type B (outdoor application) 

Speaker Component:Woofer: Min. 8.9 cm x 4, Tweeter: Max. 8.2 cm x1  

Cable Connection: Screw Terminal (Steatite), 4 ports

Material:Enclosure: Aluminium, Grill: Aluminium

Finish:White (RAL9016 or equivalent), paint

Dimension: Max. 1016 (h) x max. 124 (w) x max. 108 (d) mm

Weight:	Max. 6.7 kg