Product program / System Component / I/O Modules

U-01F

The line input module shall be unbalanced, 220k ohms with female XLR connector.

The line input module shall be TOA model U-01F.