Product program / Amplifier / System Amplifier

VM-2120   UK

<div>Microprocessor-controlled PA management amplifier, as a table top unit or with optional brackets in standard 19-inch cabinet racks can be mounted.</div><div>Three balanced inputs for microphone or recording with control inputs, height / low tone control and switchable phantom power via XLR combo jacks, transformers easily retrofitted. Input for telephone announcements. The output circuits 1-5 can be associated separately each of the above-mentioned inputs. Up to 4 auditable digital stations can be connected via an RJ-45 connection. Two audio inputs for background music with two cinch Sockets and level before controllers, as well as height / low tone control. There are 5 levels of priority. 100 V power amplifier with 120 Watt of power, idle-secure and short-circuit protected, easily convertible to 70 V or 50 v 5 output circuits, individually zuschalt-and adjustable in steps 0, - 3, 6,-10,-15 and -20 dB at any power sharing as well as a collective call key. Switching display using LEDs. In the transmission of signals with high-priority automatic bypass the volume control and display of duty call operation. Compulsory control contact for external volume control.</div><div>100V input to the 5 circles, output switchable by external duty call signal from parent PA headquarters, or switched-off device.</div><div>According an exit before and after the total volume control to the use of additional amplifiers. Recording output for the master signal.</div><div>Simple combination of two management systems to extend to 10 circuits and power increase possible.</div><div>Additional control inputs for: throwing the text rendering of the digital text storage, remote activation, start and stop of alarm texts, activation of the 100V-Eingangs.</div><div>Fault status outputs for: power and emergency power supply, receivers and amplifier combination connection, errors in the text memory.</div><div>Labels for the front taxable inputs and outputs. In emergency mode play of two texts for warning and evacuation.</div><div>Digital text storage and monitoring module can be retrofitted.</div>