Product program / Amplifier / Power Amplifier

VM-3360E  CE-GB

<div>Microprocessor-controlled extension amplifiers for voice alarm compact amplifiers with complete monitoring according to VDE 0833-4 and VDE 0828-1.</div><div>6 switchable and adjustable volume speaker outputs with a total of 360 Watt of rated output.&nbsp;</div><div>Audio input for local transmission with choice of outputs over inputs. 8 universally usable inputs and 8 universally usable control outputs; 6 separate inputs for alarm control of the BMZ with switchable monitoring, one with 24-volt control (polarity); three separate control outputs with relay contacts for feedback to the BMZ: collective fault signal (changeover contact), emergency (changeover contact) and activated CPU off (make contact). Each line output a switching relay for example external volume control in 3- and 4-wire technology.</div><div>An appropriate additional amplifier can be used as a rescue and announcement enhancer, in the second case, announcements are made without the interruption of background music in durchsagelose areas can be made. The monitoring of the additional amplifier is taken over by the extension amplifier.&nbsp;</div>