Product program / Amplifier / Power Amplifier

VP-1061   CE

<div>The amplifier shall be 1-channel power amplifier which operates on 230 -240 V AC 50/60 Hz or 24 V DC power. The specified product shall be 2U half-rack size rack-mount type, fan-cooled power amplifier. Two program inputs and two priority inputs, (both parallel, 0 dB, 20 kohm, balanced) shall be provided. The amplifier shall meet the following performance criteria: Power output shall be VP-1061: 60 W, VP-1121: 120 W at less than 1% THD (rated output, f = 1 kHz). Power consumption shall be VP-1061: 100W, VP-1121: 160W at 1/3 rated output. An output current limiter shall be provided. Frequency response shall be 80 Hz to 16 kHz at 1/3 rated output (+/-3 dB), with an S/N ratio of over 80 dB. Impedance shall be VP-1061: 167ohm (100 V), VP-1121: 83ohm (100 V). The adjustable volume level of the program input shall be attenuated whenever the priority input receives a signal. A relay contact for immediate emergency announcements shall be provided. Removable terminal blocks shall be provided for easy connection. The panel shall be black aluminum, alumite. Dimensions shall be 210 (W) x 88.4 (H) x 338.7 (D) mm and weight VP-1061: 6.9 kg, VP-1121: 9.3 kg. The operating temperature shall be 0&deg;C to +40&deg;C. Supplied accessories shall be: 2m power cable x 1, 2-pin removable terminal plug x 2, 3-pin removable terminal plug x 2, 5-pin removable terminal plug x 2, joint plate x1, joint plate mounting screw x 3, fuse (VP-1061: 1.25 A, VP-1121: 2.5 A) x 1. Fault detection of the amplifier and the speaker line shall be possible with an optional YA-1000A module. Optional rack mounting panels shall be the MB-25B-BK half-width blank panel for one amplifier unit, and the MB-25-J rack joint bracket for two units.</div><div>The power amplifier shall be TOA model VP-1061/VP-1121.</div>