Product program / Amplifier / Power Amplifier

VP-1361   CE-GB

<div>The amplifier shall be 1-channel power amplifier which operates on 230 - 240 V AC 50/60Hz or 24 V DC power. The specified product shall be 3U full rack size rack-mount, fan-cooled power amplifier. Two program inputs and two priority inputs, (both parallel, 0 dB, 20 kohm, balanced) shall be provided. The amplifier shall meet the following performance criteria: Power output shall be VP-1241: 240 W, VP-1361: 360W at less than 1% THD (rated output, f = 1 kHz). Power consumption shall be VP-1241: 240 W, VP-1361: 330 W at 1/3 rated output. An output current limiter shall be provided. Frequency response shall be 80 Hz to 16 kHz at 1/3 rated output (+/-3 dB), with an S/N ratio of over 80 dB. Impedance shall be VP-1241: 42 ohm (100 V), VP-1361: 28 ohm (100 V). The adjustable volume level of the program input shall be attenuated whenever the priority input receives a signal. A relay contact for immediate emergency announcements shall be provided. Removable terminal blocks shall be provided for easy connection. The panel shall be black aluminum, alumite. Dimensions shall be 483.6 (W) x 132.6 (H) x 337.8 (D) mm and weight VP-1241: 13.4 kg, VP-1361: 16.6 kg. The operating temperature shall be 0&deg;C to +40&deg;C. Supplied accessories shall be: 2m power cable x 1, 2-pin removable terminal plug x 2, 3-pin removable terminal plug x 2, 5-pin removable terminal plug x 2, fuse (VP-1241: 4.0 A, VP-1361: 6.3 A) x 1. Fault detection of the amplifier and the speaker line shall be possible with an optional YA-1000A module.</div><div>The power amplifier shall be TOA model VP-1241/VP-1361.</div>